Thorlabs CHROLIS - Readme 
SDK to operate the Thorlabs CHROLIS 6-Wavelength High-Power LED source from user applications.

The Chrolis device driver installer only installs the drivers for the connection between the Chrolis device and a Windows PC (USB driver, HDI driver).
The Chrolis instrument driver installer installs the device drivers and the Thorlabs instrument drivers for writing your own application (Interop, VXIPNP, LabView driver).
The Chrolis installer installs the complete package of device and instrument drivers aswell as the desktop application and the most recent firmware files. 

Note:
This software may need additional software packages to be installed for printing purposes:
	- Adobe Reader (http://www.adobe.com/reader) 

License:
This software is copyright Ó 2019 - 2024, Thorlabs GmbH. For license details please see file License.rtf.

Supported platforms:
This software was verified with the following platforms:
	- Windows 8.1 (32-bit version)
	- Windows 8.1 x64 Edition (64-bit version)
	- Windows 10 (32-bit version)
	- Windows 10 x64 Edition (64-bit version)
	- Windows 11

Change log:
V1.18	Feb-01-2020
•	Initial Release

V2.1.21	Feb-16-2022
•	Manual update includes "Write Your Own Application" instructions.

V3.0	Jul-29-2022
•	Bugfix: Switch on/off of the LEDs fails under some circumstances.
•	Bugfix: USB enabled before CHROLIS system initialization completed. Could result in user interface connection errors.
•	Introduced Round Robin Feature

V3.1	   Mar-22-2024
•	Bugfix: FW Update was not possible via the update function included in the application.