Thorlabs EXULUS - Readme 
Use this software to operate the Exulus Spatial Light Modulators (SLMs).

License:
This software is copyright ©2016-2024, Thorlabs Shanghai. For license details, please see file Thorlabs End-user License.rtf.

Supported platforms:                                                                                                                                                                                         
This software was verified with the following platforms:
 - Windows® 10 64-bit version Operating System
 - Windows® 11 64-bit version Operating System

Changelog
Changes from v2.5.3 to v2.5.4
	- Fixed an issue where the SDK files will be missing after installation. 

Changes from v2.5.1 to v2.5.3
	- Fixed an issue where saved sequence images might not be accurate.

Changes from v2.5.0 to v2.5.1
	- Added SDK for C++, LabVIEW, and Python programming environments.
	- Fixed an issue where the HDMI connection might fail.

Changes from v2.4.0 to v2.5.0
	- Added negative focal lengths for Fresnel Lens and CGH patterns.
	- Fixed an issue where previous Fresnel Lens and CGH Focal Length values might not be accurate.
	- Fixed an issue where the device might fail to connect.

Changes from v2.3.0 to v2.4.0
	- Include support for EXULUS High-Power models.
	- Include support for Internal/External thermistor reading of Liquid Chiller (item # LK220).

Changes from v2.2.1 to v2.3.0
	- Fixed an issue where the preview image does not match the actual image displayed on SLM.
	- Added a feature of "Default Setting" into Option to save the Screen Flippings and Phase Stroke Mode as default.	

Changes from v2.2.0 to v2.2.1
	- Include support for EXULUS-HD3 model.
	- Fixed an issue where some images with PNG format might fail to load.

v2.2.0
	- Initial release.
	- Supported models: EXULUS-HD2 and EXULUS-HD4.